<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.8-Bratislava">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <contact>
    <name></name>
    <organization></organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email></email>
    <role></role>
  </contact>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["RGF93 v2b / Lambert-93",BASEGEOGCRS["RGF93 v2b",DATUM["Reseau Geodesique Francais 1993 v2b",ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",9782]],CONVERSION["Lambert-93",METHOD["Lambert Conic Conformal (2SP)",ID["EPSG",9802]],PARAMETER["Latitude of false origin",46.5,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8821]],PARAMETER["Longitude of false origin",3,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8822]],PARAMETER["Latitude of 1st standard parallel",49,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8823]],PARAMETER["Latitude of 2nd standard parallel",44,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8824]],PARAMETER["Easting at false origin",700000,LENGTHUNIT["metre",1],ID["EPSG",8826]],PARAMETER["Northing at false origin",6600000,LENGTHUNIT["metre",1],ID["EPSG",8827]]],CS[Cartesian,2],AXIS["easting (X)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["northing (Y)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["France - onshore and offshore, mainland and Corsica (France métropolitaine including Corsica)."],BBOX[41.15,-9.86,51.56,10.38]],ID["EPSG",9794]]</wkt>
      <proj4>+proj=lcc +lat_0=46.5 +lon_0=3 +lat_1=49 +lat_2=44 +x_0=700000 +y_0=6600000 +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>64102</srsid>
      <srid>520004102</srid>
      <authid>EPSG:9794</authid>
      <description>RGF93 v2b / Lambert-93</description>
      <projectionacronym>lcc</projectionacronym>
      <ellipsoidacronym>EPSG:7019</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial miny="0" maxz="0" minz="0" maxx="0" maxy="0" minx="0" crs="EPSG:9794" dimensions="2"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
